**Suggested Specification Guidelines for Gage Ceilings D3**

Specifying Gage Ceilings is a simple process. Follow the guidelines listed below. Complete architectural (Technical) specifications and installation guidelines can be downloaded from our website at [www.gagecorp.net](http://www.gagecorp.net) or contact the factory.

**Item**: Gage Decorative Metal Ceilings / Profile System D3

**Design**:

Enter specified design, i.e. design #250

**Profile:**  D3.1 Flush flat  D3.2 Coffer flat

D3.3 Tegular flat (3/8” reveal edge)

D3.4 Coffer regular

D3.5 Tegular flat for 9/16” T-grid (3/8” reveal edge)

**Size**: 24” x 24” nominal

**Finish:**

(Gloss levels from 30 – 100% +/- 5%)

**Flame Spread:** Class 1, ASTM E84

**Metal:** .030” aluminum (at least 50% recycled)

**Optional**:  NRC: 0.75 flat profile perforated panel

NRC 0.52 coffered profile perforated panel

(perforation with acoustical membrane)

**Suspension:** Refer to Section 09120